Sound integration:

The following method will integrate the pressure of a point.

Take all points on the sphere at radius ct, where c is the speed of sound and t is the time differential. The total pressure at the center at time t is equal to the average contribution from each point, where the contribution is the pressure plus the distance times gradient with respect to the distance, plus the time times the gradient with respect to time.